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 Metal Roof Refurbishment works at Power Centre and Sheds at SSRIA


Procurement Ref: ONB/WK/TSD/VB/CL/25/008 RL1 (14 OCT 26) TC
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…. August 2026


Dear Sir;/Madam

Airports of Mauritius Co Ltd (AML) is inviting you to submit your bid for the Metal Roof Refurbishment works at Power Centre and Sheds at SSRIA, as described in this bidding document.

We commit ourselves to maintain the highest standard of integrity and ethical principles during all stages of the procurement cycle.

You are kindly requested to submit the following documents together with your bid, but not limited to:

1. Duly filled Bid Submission Form
2. Duly filled Priced Bill of Quantities
3. Duly filled Qualification Information Form and attachments required
4. Report on the financial standing of the Bidder for the last three years, such as certified copies of Financial Statements or Audited Accounts as filed at the Registrar of Companies before the deadline set for submission of bids
5. Valid Registration Certificate with the CIA, as applicable
6. Signed C.V of Site Agent
7. Documentary evidence of liquid assets and/or credit facilities
8. Any other documents deemed necessary as per the requirements of this bidding document.

We thank you for your kind consideration.

Yours faithfully






Chairperson Tender Committee
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Section I: Instruction to Bidders

1. Introduction

Airports of Mauritius Co Ltd (AML) also referred as the Employer, invites eligible local Contractors to submit their bid for the works detailed in this bidding document. 

Any resulting Contract shall be subject to the Terms and Conditions stipulated in this document.

The project consists of the Metal Roof Refurbishment works at Power Centre and Sheds at SSRIA.

1.1 Clarifications (if any), should be addressed to the Chairperson Tender Committee, SSR International Airport, Plaine Magnien, and sent through email at: tendercommittee@aml.aero

AML will respond in writing to any request for clarification, provided that such request is received 14 calendar days prior to the deadline for submission of bids. 

Bidders are requested to visit regularly the AML Website, so as to take cognizance of any Addendum/Clarifications issued and uploaded therein.

Late bids shall not be accepted and bids submitted by any electronic mode shall not be considered. 

1.2 Bidders are advised to carefully read the complete bidding document, including the Particular Conditions of Contract in Section IV, before preparing their bids. 

The standard forms in this document may be retyped for completion, but the bidder shall be solely responsible for their accurate reproduction.

2. Validity of bids

The bid shall valid for 120 calendar days from the bid submission date. 

3. Works Completion Period

The Intended Completion period for the Works shall be 90 calendar days from the start date specified in the Notice to Commence.  

4. Site Visit (Mandatory)

Bidders or their designated representatives are invited to attend a site visit on Tuesday 08 September 2026 at 10h00. 

The venue shall be AML Meeting Room, Ground Floor, AML Corporate Office, Plaine Magnien. 
Bidders should confirm their participation to the Secretary Tender Committee on 603-6000 or through email at tendercommittee@aml.aero, at least 24 hours prior to pre-bid/site visit, for access permit purposes.  

Bidders are required to attend the mandatory site visit in order to gain a clear understanding of the nature, scope, complexity, and operational constraints associated with the works within the airport environment. The site visit will enable bidders to familiarize themselves with site conditions, access restrictions, safety requirements, operational interfaces, and all applicable airport regulations and procedures, thereby allowing them to submit a comprehensive and competitive offer.

5. Sealing and Marking of Bids

Bids should be properly sealed in a single envelope, clearly marked with the Procurement Reference, addressed to the Chairperson Tender Committee with the Bidder’s name at the back of the envelope.

6. Submission of Bids

Bids should be deposited in the Tender Box located at the Ground Floor, AML Corporate Office, SSR International Airport, Plaine Magnien on or before Wednesday 14 October 2026 at latest by 13h00. Bidders are also informed that, in case the deadline to submit bid is a non-working day, tacitly, the next working day shall be the Closing Date and at the same time.

Bids sent by registered post or hand delivered should reach the above-mentioned address by the same date and time as prescribed above.  

Late bids shall not be accepted and bids submitted by any electronic mode shall not be considered.

7. Bid Opening

[bookmark: _GoBack]Bids will be opened by AML Tender Committee in the Meeting Room, Ground Floor, AML Corporate Office, SSR International Airport, Plaine Magnien on Wednesday 14 October 2026 at 13h30. 

Bidders or their delegated representatives may attend the Bid Opening exercise if they choose to do so. One representative per bidder shall be allowed for the bid opening exercise.

Bidders should confirm their participation to the Secretary Tender Committee on 603- 6000 or through email at tendercommittee@aml.aero

8. Eligibility Criteria

To be eligible to participate in this bidding exercise, Bidder should:

(a) have the legal capacity to enter into a contract to execute the works;
(b) be duly registered with the CIA under the grade that would allow him to perform the value of works for which he is submitting his bid (Note 1). 
(c) not be insolvent, in receivership, bankrupt, subject to legal proceedings for any of    these circumstances or in the process of being wound up; 
(d) not have had your business activities suspended;
(e) not be under a declaration of ineligibility by the Government of Mauritius in accordance with applicable laws at the date of the deadline for bid submission or appearing on the ineligibility lists of African Development Bank, Asian Development Bank, European Bank for Reconstruction and Development, Inter-American Development Bank Group and World Bank Group;
(f) not have a conflict of interest in relation to this procurement requirement; and
(g) have a Business Registration Card.

Note 1: Sub-contractors undertaking works are also subject to registration with CIA as applicable to Contractors.

9. Qualification and Experience Criteria

Bidders should have the following minimum qualifications and experience:

(a) successfully completed as Prime Contractor at least 2 projects of a similar nature and complexity over the last 5 years.
(b) Site Agent with minimum qualification of diploma in building/civil engineering and at least 5 years’ in the related field/equivalent nature and complexity. 
(c) Staff qualified for working at height.

Note 2: At time of bidding and for evaluation purposes, bidders are requested to submit the following documentary evidence:

· List of similar projects completed as Prime Contractor
· Qualifications and experience of above key personnel

10. Contents of Bid

The Bid shall comprise the following:

(a) duly filled Bid Submission Form
(b) duly filled Priced Bill of Quantities
(c) duly filled Qualification Information Form and attachments required
(d) report on the financial standing of the Bidder for the last three years, such as certified copies of Financial Statements or Audited Accounts as filed at the Registrar of Companies before the deadline set for submission of bids
(e) Valid Registration Certificate with the CIA, as applicable
(f) Signed C.V of Site Agent
(g) Documentary evidence of liquid assets and/or credit facilities
(h) Any other documents deemed necessary as per the requirements of this bidding document.

Note 3: Bidders to demonstrate access to, or availability of Financial Resources such as Liquid Assets, Lines of Credit, and other financial means, other than any Contractual advance payments to meet the overall cash flow requirements for the Contract and its current commitments.

Documentary evidence may comprise, but not limited to, Bank Certificate, Certificate from Auditors, Certificate from a Professional Accountant registered with MIPA.
11. Prices and Currency of payment

Bidders should quote for the whole works. Prices for the execution of works shall be quoted and fixed, in Mauritian Rupees. Items for which no rate or price is entered by bidders, shall not be paid for by AML when executed and shall be deemed to be included/apportioned by the other rates and prices in the Bill of Quantities.

Bids shall cover all costs of labour, materials, equipment, overheads, profits and all associated costs for performing the works, and shall include all duties.

The whole cost of performing the works shall be included in the BOQs, and the cost of any incidental works shall be deemed to be included in the prices quoted. 

12. Bid Securing Declaration

Bidders are required to subscribe to a Bid Securing Declaration (BDS) as per attached BDS Form.

13. Margin of Preference

Not applicable

14. Evaluation of Bids

AML shall have the right to request for clarification during evaluation. Bids which are substantially responsive to the requirements, shall be compared on the basis of price proposed, to determine the lowest evaluated bid.

If the lowest evaluated bid is seriously unbalanced or front loaded or if any item in the Bill of Quantities or Price Schedule is front loaded or contains an erroneous amount in the opinion of the Employer, the Employer may require the Bidder to produce detailed price analysis for any or all items of the bid to demonstrate the internal consistency of those prices with the construction methods and schedule proposed. After analysis of the prices the Employer may reject the bid or require that the amount of the Performance Security be increased at the expense of the Bidder to a level sufficient to protect the Employer against financial loss in the event of default of the successful Bidder under the Contract.

15. Award of Contract

The Bidder having submitted the lowest evaluated responsive bid and qualified to perform the works shall be selected for award of Contract. Award of Contract shall be by issue of a Letter of Acceptance in accordance with Terms and Conditions contained in Section IV: General Conditions of Contract and Particular Conditions of Contract.

16. Performance Security and Signing of Contract

The Successful Bidder shall, within 28 calendar days of the issue date of the Letter of Acceptance, submit a Performance Security from a Commercial bank operating in Mauritius, of 10% of Contract Value (excluding any Provisional and contingency sums and excluding VAT) which shall be valid up to 28 calendar days following the end of the contract period. 

The Contract Agreement shall be signed within 28 calendar days after the successful bidder receives the Letter of Acceptance unless the parties agree otherwise.

17. Notification of Award and Debriefing

		Airports of Mauritius Co Ltd shall after award of contract, exceeding MUR 1 Million, promptly inform all unsuccessful bidders in writing of the name and address of the successful bidder and the contract amount.

	Furthermore, Airports of Mauritius Co Ltd shall attend to all requests for debriefing for contract exceeding MUR 1 Million, made in writing within 30 calendar days the unsuccessful bidders are informed of the award.

18. Advance Payment

AML shall provide an Advance Payment on the Contract Price as stipulated in the General Conditions of Contract. The Advance Payment shall be guaranteed by an Advance Payment Security, as per the format contained in Section V.

The Advance Payment shall be limited to 10% percent of the Contract Price, less any provisional and contingencies sums but excluding VAT.

19. Integrity Clause

AML commits itself to take all measures necessary to prevent corruption and ensures that none of its staff, personally or through his/her close relatives or through a third party, will in connection with the bid for, or the execution of a Contract, demand, take a promise for or accept, for him/herself or third person, any material or immaterial benefit which he/she is not legally entitled to.

20. Rights of AML

Airports of Mauritius Co. Ltd shall have the right to;

(a) seek clarifications at time of evaluating quotations;
(b) negotiate with the preferred bidder; 
(c) reject all quotations and;
(d) cancel the whole bidding exercise without incurring any liability to the bidders. 

Airports of Mauritius Co. Ltd shall not be bound to accept the lowest or any quotation.

21. Challenge and Appeal

The address to file Challenges in respect of this procurement is:

The Chief Executive Officer
Airports of Mauritius Co. Ltd
AML Corporate Office
Sir Seewoosagur Ramgoolam International Airport
Plaine Magnien 51520
Mauritius
Tel: +230 603 6000
Email : secretarytoceo@aml.aero 

Section II: Bidding Forms

Note: Bidders are required to fill all the forms in this section and submit as part of their bid. Non- submission of any form may lead to rejection of the bid
Bid Submission Form

Date: 		 Bid’s Reference No.: 	 Procurement Reference No:……………………

To:

We, the undersigned, declare that:

(a) We have examined and have no reservations to the Bidding Documents, including Addenda issued;
(b) We offer to execute in conformity with the Bidding Documents the following Works:
	;
(c) The total price of our Bid excluding VAT is: 	(MUR):

(d) Our bid shall be valid for a period of 120 calendar days from the date fixed for the bid
submission deadline in accordance with the Bidding Documents or up to	,
whichever is later, and it shall remain binding upon us and may be accepted at any time before the expiration of that period;
(e) We hereby confirm that we have read and understood the content of the Bid Securing Declaration attached hereto and subscribe fully to the terms and conditions contained therein, if required. We understand that non-compliance to the conditions mentioned may lead to disqualification.
(f) If our bid is accepted, we commit to submit a Performance Security in accordance with the Terms and Conditions;
(g) We, including any SubContractors or suppliers for any part of the Contract, do not have any conflict of interest in accordance with ITB 9;
(h) We are not participating, as a bidder in more than one bid in this bidding process;
(i) Our firm, its affiliates or subsidiaries, including any SubContractors or Suppliers for any part of the Contract, has not been declared ineligible under the laws of Mauritius;
(j) We have taken steps to ensure that no person acting for us or on our behalf will engage in any type of fraud and corruption as per the principles described hereunder, during the bidding process and Contract execution:

i. We shall not, directly or through any other person or firm, offer, promise or give to any of the AML’s employees involved in the bidding process or the execution of the Contract or to any third person any material or immaterial benefit which he/she is not legally

entitled to, in order to obtain in exchange any advantage of any kind whatsoever during the tender process or during the execution of the Contract.
ii. We shall not enter with other bidders into any undisclosed agreement or understanding, whether formal or informal. This applies in particular to prices, specifications, certifications, subsidiary Contracts, submission or non-submission of bids or any other actions to restrict competitiveness or to introduce cartelisation in the bidding process.
iii. We shall not use falsified documents, erroneous data or deliberately not disclose requested facts to obtain a benefit in a procurement proceeding.
We understand that transgression of the above is a serious offence and appropriate actions will be taken against such bidders.

(k) We understand that this bid, together with your written acceptance, shall constitute a binding Contract between us, until a formal Contract is prepared and executed;
(l) We understand that you are not bound to accept the lowest evaluated bid or any other bid that you may receive; and
(m) If awarded the Contract, the person named below shall act as Contractor’s Representative:

 	Name:
In the capacity of:
Signed:
Duly authorized to sign the Bid for and
on behalf of:
Date:
Seal of Company:


 	
 	


 	
 	
 	



Appendix to Bid Submission Form


BID SECURING DECLARATION

By subscribing to the undertaking in the Bid Submission Form: 
I/We accept that I/we may be disqualified from bidding for any contract with Airports of Mauritius Co. Ltd for the period of time that may be determined by the Procurement Policy Office under section 35 of the Public Procurement Act, if I am/we are in breach of any obligation under the Bid conditions, because I/we:
(a) have modified or withdrawn my/our bid after the deadline for submission of bids during  the period of bid validity specified by the Bidder in the Bid Submission Form; or
(b) have refused to accept a correction of an error appearing on the face of the bid; or
(c) having been notified of the acceptance of our bid by the Airports of Mauritius Co. Ltd during the period of bid validity, (i) have failed or refused to execute the Contract, if required, or (ii) have failed or refused to furnish the Performance Security, in accordance with the Instructions to Quote.
I/We understand this Bid Securing Declaration shall cease to be valid (a) in case I/we am/are  the successful bidder, upon our receipt of copies of the contract signed by you and the Performance Security issued to you by me/us ; or (b) if I am/we are not the successful Bidder, upon the earlier of (i) the receipt of your notification of the name of the successful Bidder; or (ii) thirty days after the expiration of the validity of my/our bid.

* To delete as appropriate. 

	Name of Bidder
	
	Company’s Address and seal

	
	
	

	Contact Person
	
	

	Name of Person Authorising the Quotation:

	Position:
	Signature:

	Date
	
	Phone No./E-mail
	




Qualification Information


	1. Individual Bidders or Individual Members of
Joint Ventures
	1.1	Constitution or legal status of Bidder: [attach copy]
Place of registration: [insert] Principal place of business: [insert]




1.2 Bidder shall provide least 2 projects of a nature and amount similar to the Works performed as prime Contractor over the last  5 years.

	Project/Contract name
and country
	Name of client and
contact person
	Type of work performed
and year of completion
	Value of Contract
(national currency )

	(a)

(b)
	
	
	




1.3 Proposed subContracts and firms involved. Refer to General Conditions of Contract Clause 7.


	Sections of the Works
	Value of
subContract
	SubContractor
(name and address)
	Experience in similar work

	(a)

(b)
	
	
	



[Bidders have to ascertain that sub-Contractors executing works are duly registered with the CIA].


1.4 Name, address, and telephone, telex, and facsimile numbers of banks that may provide references if contacted by AML.



2. Additional

2.1 Bidders should provide any additional information Requirements requested in the bidding document. 
Bill of Quantities

Procurement Reference Number: ONB/WK/TSD/VB/CL/25/008 RL1 (14 Oct) TC

BILL NO. 1: NEW ROOF METAL SHEETING TO SEWER TREATMENT PLANT SHELTER - (LOT 1)

Refer to Dwg no. AML/AWWD/01, 02, 03, 04

	ITEM
NO.
	DESCRIPTION
	UNIT
	RATE (MUR) (Excl. VAT)
	AMOUNT (MUR) 
(Excl. VAT)

	1.0
	DISMANTLING WORKS

	 
	Dismantling of existing Metal sheeting as described below and handover to Client or cart away from site to an approved dumping site within 2 km of site unless otherwise specified.  Contractor shall allow for temporary hoarding and protections as may be required to existing structures.  No stacking of debris and the like will be allowed outside the areas allocated to the contractor.  
	 
 
	 
	 

	1.1
	Metal sheets including Capping, Flashing and all fixation fittings, screws and left clean to receive new Sheeting. 
	SUM
	 
	 

	 
	SUBTOTAL 1 (Dismantling)

	 

	2.0
	PRELIMINARY & GENERAL

	2.1
	Allow for installations, mobilisation, demobilisation including electricity, potable water, lighting, Scaffolding and area demarcations. Allowance also to be made for survey of existing Structure.
	SUM
	 
	 

	2.2
	Allow for compliance with AML Co. Ltd regulations in terms of health & safety, security, environmental impact, access permit and interfacing with authorities, etc.
	SUM
	 
	 

	2.3
	Contractor shall include in this Bill for all cost he considers deemed to be necessary P&G items and to complete the project.
	SUM
	 
	 

	 
	SUBTOTAL 2 (P&G Cost)

	 

	
	AMOUNT C/F

	



54	


	ITEM
NO.
	DESCRIPTION
	UNIT
	QTY
	RATE (MUR) (Excl. VAT)
	AMOUNT (MUR)
(Excl. VAT)

	
	AMOUNT B/F
	

	3.0
	NEW WORKS

	 
	Roof Sheeting 

	
	Galvanised mild steel  roof sheeting 0.75mm thick prepainted both sides or equal approved, profiled to Client's approval, complete with all fixings devices including approved self tapping screws, washers, caps and malakoffs, side and en laps sealed with waterproof adhesive strips, including all necessary cutting with Nibbler Cutter, waste and protection, all to manufacture's specification and Client's approval.
	
	
	
	

	3.1
	Roof covering with pitch
	m2
	54
	 
	 

	3.2
	Extra over for crimping of sheets
	Lm
	8
	 
	 

	 
	GMS Capping/Flashing 0.75mm thick prepainted sheeting 600mm girth; with and including all fixings waterproof bands tape, self adhesive foam closure strips along both sides of flashing and standard closer to underside, all to manufacture's specification and Client's approval.
	 
	 
	 
	 

	3.3
	Hip Capping
	Lm
	8
	 
	 

	3.4
	Hip Flashing
	Lm
	8
	 
	 

	3.5
	Barge Capping
	Lm
	18
	 
	 

	 
	The following in hot dipped galvanised after manufacture mild steel.  Rate to include for cutting to sizes, rounding sharp edges, continuous fillet welds where required, brush galvanising of site welds and fixing with appropriate bolts.  Rate to include for application of one coat of galvanised iron cleaner, one coat of etch primer and two coats of enamel paint.
	
	
	 
	 

	3.6
	Supply and fix of METAL C-PULINS size: 100X 100 X 2.4mm thick.
	Lm
	30
	 
	 

	3.7
	Manufacture, Supply and fix of METAL PLATES size: 100X 100 X 5mm thick. Including of fillet welding of 6mm all along, Connection/ Anchor Bolts M12, washers, nuts. Rate to include for application of one coat of galvanised iron cleaner, one coat of etch primer and two coats of enamel paint. as per Drawings and Client Approval.
	Nr
	24
	 
	 

	 
	SUBTOTAL 3 (New Work)
	 

	 SUBTOTAL  (Contingency)
	50,000.00

	 TOTAL AMOUNT (LOT 1) (Excl. VAT)
	 	


	
Signature of Bidder: …………………………………………………………

	
	
	
	
	

	Company Seal:
	
	
	



Procurement Reference Number: ONB/WK/TSD/VB/CL/25/008 RL1 (14 Oct) TC

BILL NO. 2: NEW METAL SHEETING AT POWER CENTRE - (LOT 2)

REFER Dwg No. AML/PCR/01

	ITEM
NO.
	DESCRIPTION
	UNIT
	RATE (MUR) (Excl. VAT)
	AMOUNT (MUR) 
(Excl. VAT)

	1.0
	DISMANTLING WORKS

	 
	Dismantling of existing Metal Elements as described below and handover to Client or cart away from site to an approved dumping site within 2 km of site unless otherwise specified.  Contractor shall allow for temporary hoarding and protections as may be required to existing structures.  No stacking of debris and the like will be allowed outside the areas allocated to the contractor.  
	 
 
	 
	 

	1.1
	Including Louvers, Flashing, Metal sheets and all fixation fittings, screws and left clean to receive new Sheeting. 
	SUM
	 
	 

	 
	
SUBTOTAL 1 (Dismantling) 
	 

	2.0
	PRELIMINARY & GENERAL

	2.1
	Allow for installations, mobilisation, demobilisation including electricity, potable water, lighting, Scaffolding and area demarcations. Allowance also to be made for survey of existing Structure.
	SUM
	 
	 

	2.2
	Allow for compliance with AML Co. Ltd regulations in terms of health & safety, security, environmental impact, access permit and interfacing with authorities, etc.
	SUM
	 
	 

	2.3
	Contractor shall include in this Bill for all cost he considers deemed to be necessary P&G items and complete the project.
	SUM
	 
	 

	 
	
SUBTOTAL 2 (P&G Cost)
	 

	
	
AMOUNT C/F
	



	ITEM
NO.
	DESCRIPTION
	UNIT
	QTY
	RATE (MUR) (Excl. VAT)
	AMOUNT (MUR)
(Excl. VAT)

	
	AMOUNT B/F
	

	3.0
	NEW WORKS

	 
	Metal Sheeting

	 
	Galvanised mild steel  roof sheeting 0.75mm thick prepainted both sides or equal approved, profiled to Client's approval, complete with all fixings devices including approved self tapping screws, washers, caps and malakoffs, side and en laps sealed with waterproof adhesive strips, including all necessary cutting with Nibbler Cutter, waste and protection, all to manufacture's specification and Client's approval.
	 
	 
	 
	 

	3.1
	Roof covering with pitch to front of louvers
	m2
	80
	 
	 

	3.2
	Behind louvered Vents -1300mm wide
	m2
	52
	 
	 

	3.3
	Included Canopy -600mm wide
	m2
	24
	 
	 

	 
	GMS Capping/Flashing 0.75mm thick prepainted sheeting 600mm girth; with and including all fixings waterproof bands tape, self adhesive foam closure strips along both sides of flashing and standard closer to underside , all to manufacture's specification and Client's approval.
	 
	 
	 
	 

	3.4
	Cap Flashing to metal sheet screen
	Lm
	40
	 
	 

	3.5
	Flashing to U Shape Purlins
	Lm
	40
	 
	 

	 
	Gutter under metal louvers
	 
	 
	 
	 

	 
	Manufactured, supply and fix of coated colour  aluminium Gutter  to Contractor's design and in line with existing design .  Aluminium Gutter shall made of 3.5mm thick including all necessary stiffeners and GMS metal Brackets of 25mm x5mm thick. All to be as per Clients Approval.
	 
	 
	 
	 

	3.6
	Aluminium gutter, girth not exceeding 600mm 
	Lm
	40
	 
	 

	 
	Existing Metal Elements:
	 
	 
	 
	 

	 
	Refix of existing elements to original position, including of Cleaning, sanddown and apply of one coat of galvanised iron cleaner, one coat of etch primer, two coat of enamel Gloss paint and to be fixed with new appropriate bolts / fixation fittings.
	 
	 
	 
	 

	3.7
	Existing Metal Louvers:
	Lm
	40
	 
	 

	3.8
	Existing Barge flashing (underneath of front louvers)
	Lm
	40
	 
	 

	
	AMOUNT C/F

	



	ITEM
NO.
	DESCRIPTION
	UNIT
	RATE (MUR) (Excl. VAT)
	AMOUNT (MUR)
(Excl. VAT)

	
	AMOUNT B/F

	

	4.1
	Chipping of rust to existing metallic Structure, including of apply of one coat of galvanised iron cleaner, one coat of etch primer as per Engineer's / Client approval.
	Sum
	 
	50,000.00

	4.2
	Remove of all rusty Bolts, washers & nuts and Replace with new Galvanised Steel Bolts, Washers & nuts to same designed dimensions. As per Engineer's/ Client approval.
	Sum
	 
	50,000.00

	4.3
	Anti Bird Netting, Supply and fix of PVC mesh netting to Metal Louvers, including of GMS press Plat (20mm x 3mm thk)  As per Engineer's/ Client approval.
	Item
	 
	100,000.00

	 SUBTOTAL 3 (New Work)
	 

	 SUBTOTAL 4 (Contingency) 
	135,000.00

	 TOTAL AMOUNT (LOT 2) (Excl. VAT)
	 	





	
Signature of Bidder: …………………………………………………………

	
	
	
	
	

	Company Seal:
	
	
	




Procurement Reference Number: ONB/WK/TSD/VB/CL/25/008 RL1 (14 Oct) TC

BILL NO. 3: NEW ROOF METAL SHEETING AT GROUND2AIR WORKSHOP - (LOT 3)

	ITEM
NO.
	DESCRIPTION
	UNIT
	RATE (MUR) (Excl. VAT)
	AMOUNT (MUR)
(Excl. VAT)

	1.0 
	DISMANTLING WORKS

	
	Dismantling of existing Metal sheeting as described below and handover to Client or cart away from site to an approved dumping site within 2 km of site unless otherwise specified.  Contractor shall allow for temporary hoarding and protections as may be required to existing structures.  No stacking of debris and the like will be allowed outside the areas allocated to the contractor.  
	
	 
	 

	1.1
	Metal sheets including Capping, Flashing and all fixation fittings, screws and left clean to receive new Sheeting. 
	SUM
	
	

	
	SUBTOTAL 1 (Dismantling)

	

	2.0
	PRELIMINARY & GENERAL

	2.1
	Allow for installations, mobilisation, demobilisation including electricity, potable water, lighting, scaffolding and area demarcations. Allowance also to be made for survey of existing Structure.
	SUM
	
	

	2.2
	Allow for compliance with AML Co. Ltd regulations in terms of health & safety, security, environmental impact, access permit and interfacing with authorities, etc.
	SUM
	
	

	2.3
	Contractor shall include in this Bill for all cost he considers deemed necessary P&G items and to complete the project.
	SUM
	
	

	
		SUBTOTAL 2 (P&G Cost)

	

	
	AMOUNT C/F

	



	ITEM
NO.
	DESCRIPTION
	UNIT
	QTY
	RATE (MUR) (Excl. VAT)
	AMOUNT (MUR)
(Excl. VAT)

	
	AMOUNT B/F
	

	3.0
	NEW WORKS

	 
	Roof Sheeting
	 
	 
	
	

	 
	Galvanised mild steel  roof sheeting 0.75mm thick prepainted both sides or equal approved, profiled to Client's approval, complete with all fixings devices including approved self tapping screws, washers, caps and malakoffs, side and en laps sealed with waterproof adhesive strips, including all necessary cutting with Nibbler Cutter, waste and protection, all to manufacture's specification and Client's approval.
	 
	 
	
	

	3.1
	Roof covering with pitch
	m2
	108
	
	

	3.1
	to Side wall RHS
	m2
	13
	
	

	3.1
	to Side wall LHS
	m2
	30
	
	

	3.2
	to End wall
	m2
	47
	
	

	 
	GMS Capping/Flashing 0.75mm thick prepainted sheeting 600mm girth; with and including all fixings waterproof bands tape, self adhesive foam closure strips along both sides of flashing and standard closer to underside , all to manufacture's specification and Client's approval.
	
	
	
	

	3.3
	Barge Capping  to LHS Side wall -girth n.e 700mm
	Lm
	30
	
	

	3.4
	Bottom flashing to LHS Side wall-  girth  n.e 400mm
	Lm
	39
	
	

	3.5
	Gutter to Front elevation-  girth  n.e 400mm  including of 6nr spout for rainwater down pipe.
	Lm
	36
	
	

	 
	The following in hot dipped galvanised after manufacture mild steel.  Rate to include for cutting to sizes, rounding sharp edges, continuous fillet welds where required, brush galvanising of site welds and fixing with appropriate bolts.  Rate to include for application of one coat of galvanised iron cleaner, one coat of etch primer and two coats of enamel paint.
	 
	 
	
	

	3.6
	Supply and fix of METAL Z-PULINS size: 180X 50 X 2.4mm thick.- to RHS Side Wall
	Lm
	39
	
	

	3.7
	Supply and fix of METAL Z-PULINS size: 180X 50 X 2.4mm thick.- to  LHS Side Wall
	Lm
	39
	
	

	
	AMOUNT C/F

	



	ITEM
NO.
	DESCRIPTION
	UNIT
	QTY
	RATE (MUR) (Excl. VAT)
	AMOUNT (MUR)
(Excl. VAT)

	
	AMOUNT B/F
	

	3.8
	Supply and fix of METAL Z-PULINS size: 250X 90 X 2.4mm thick.- to  LHS End Wall
	Lm
	144
	
	

	3.9
	Supply and fix of METAL Z-PULINS size: 250X 90 X 2.4mm thick.- to  Roof
	Lm
	125
	
	

	3.10
	Supply and fix of METAL Z-PULINS size: 250X 90 X 2.4mm thick.- to Front
	Lm
	36
	
	

	4.1
	Chipping of rust to existing metallic Structure, including of apply of one coat of galvanised iron cleaner, one coat of etch primer as per Engineer's / Client approval.
	Sum
	
	50,000.00

	4.2
	Remove of all rusty Bolts, washers & nuts and Replace with new Galvanised Steel Bolts, Washers & nuts to same designed dimensions. As per Engineer's/ Client approval.
	Sum
	
	50,000.00

	 
	SUBTOTAL 3 (New Work)
	

	 SUBTOTAL  (Contingency)
	200,000.00

	 TOTAL AMOUNT (LOT 3) (Excl. VAT)
	




	
Signature of Bidder: …………………………………………………………

	
	
	
	
	

	Company Seal:
	
	
	



	Metal Roof Refurbishment works at Power Centre and Sheds at SSRIA


	BILL OF QUANTITES - MAIN SUMMARY OF PRICES



	 Bill No.
	General Summary
	Amount (MUR)

	1
	Total for Bill No. 1: 
New Roof Metal Sheeting to Sewer Treatment Plant Shelter – Lot 1
	

	2

	Total for Bill No. 2:
New Metal Sheeting at Power Centre – Lot 2
	

	3
	Total for Bill No. 3:
New Roof Metal Sheeting at Ground2Air Workshop - |Lot 3
	

	4
	Performance Security for Lots 1, 2 and 3

	

	5
	Advance Payment Guarantee for Lots 1, 2 and 3

	

	 SUB TOTAL (Excl. VAT)
 
	

	ADD VAT AT 15%
	

	TOTAL AMOUNT INCLUDING ALL CHARGES
	



Bill of Quantities Authorised By:

	Name:
	
	Signature:
	

	Position:
	
	Date:
	

	Authorised for and on behalf of:
	Company:
	









48	Section IV- Priced Activity Schedule


KEY FINANCIAL INFORMATION FORM

Key Financial Information extracted from Audited Accounts/Financial Statements
	Financial   data in the currency reported in the Audited Accounts / Financial Statements
	Historical Information
	Remarks by BEC

	
	Previous years
	Last year
	Current year
	

	Statement of Financial Position (Information from Balance Sheet) 
	

	A. Current Assets 
	 
	 
	 
	

	B. Current Liabilities 
	 
	 
	 
	

	Working capital ratio or current ratio (A/B) 
	 
	 
	 
	

	Quick ratio or Acid Test ratio 
(Current Asset net of stock /B) 
(A – Closing Stock)
            B
	 
	 
	 
	

	C. Total Assets 
	 
	 
	 
	

	D. Total Liabilities  
	 
	 
	 
	

	Net Asset  ( C-D) 
	 
	 
	 
	

	Cash in hand and at Bank 
	 
	 
	 
	

	Bank Overdrafts  
	 
	 
	 
	

	Other Liquid Assets  
	 
	 
	 
	

	Debt to Equity Ratio (Gearing / Solvency ratio) Long Term Debt X100
                  Equity  
	
	
	
	

	Information from Income statement

	Key Profitability Indicators in  the currency reported in the Audited Accounts/Financial Statements 
	Previous years
	Last year
	Current year
	

	Turnover 
	 
	 
	 
	

	Profit /(Loss )Before Tax 
	 
	 
	 
	

	Taxation  
	 
	 
	 
	

	Net Profit /(Loss) After Tax 
	 
	 
	 
	

	(Net profit After tax) x 100 
(Turnover) 
	 
	 
	 
	

	 Certified by Bidder that information is true extract from Audited Accounts/ Financial Statements
 Name of Bidder: 

 Signature: 
 
Capacity: 
 
Date: 



Financial Resources
Form FIN 3.3

Specify proposed sources of financing, such as liquid assets, unencumbered real assets, lines of credit, and other financial means, net of current commitments, available to meet the total construction cash flow demands of the subject contract or contracts as indicated in Section III (Evaluation and Qualification Criteria).

	Source of financing
	Amount (MUR  equivalent)

	1.

	

	2.

	

	3.

	

	4.

	






Section III: Statement of Requirements

A. SCOPE OF WORKS AND PERFORMANCE REQUIREMENTS

The scope of works comprises of Metal Roof Refurbishment works at Power Centre and Sheds at SSRIA. The Contractor shall execute all works in accordance with the specifications, drawings, and Employer’s requirements, ensuring operational continuity of the Airport and compliance with AML’s Health & Safety standards.

GENERAL OBLIGATIONS 

· Provision of insurance coverage and compliance with contractual obligations.

· Facilitation of site access, including DCA permits, Certificates of Character, and work permits.

· Provision and erection of scaffoldings, as per the Occupational Safety and Health Act.

· Compliance with AML and local Health & Safety regulations.

· Provision of temporary utilities, hoardings, and protection of existing structures.

· Site cleaning, setting out, and submission of project documentation (methodology, work plans, as-built drawings, etc.).

· Installation of sign boards and traffic diversion measures.

· The Contractor shall provide valid Working at Height certificates and relevant training records for all personnel engaged in works at elevated levels. Copies of certificates shall be submitted to the Client/Engineer prior to commencement of works on site.

· The Contractor shall submit a detailed Method Statement and Work Plan for all sites prior to commencement of works. The submission shall clearly indicate the proposed phasing of works, sequence of activities, access arrangements, safety measures and associated risks (Risk Assessment) together with mitigation measures for review and approval by the Client/Engineer.


SCOPE OF WORKS

LOT 1 – NEW METAL SHEETING TO SEWER TREATMENT PLANT SHELTER

1. DISMANTLING WORKS

1.1 General

Carefully dismantle existing metal sheeting and associated accessories as described below and hand over reusable materials to the Client or cart away debris to an approved dumping site within 2 km from site unless otherwise specified.
The Contractor shall allow for:

· Temporary hoarding and protection to existing structures and surrounding installations.
· Safe removal and disposal of debris.
· No stacking of debris or dismantled materials outside allocated working areas.
· Leaving all surfaces clean and ready to receive new works.

1.2 Existing Metal Roofing Elements

The works shall include dismantling and removal of:

· Existing metal roof sheets
· Existing capping
· Existing flashing
· Existing fixation fittings, screws and accessories

2. PRELIMINARY & GENERAL

2.1 Site Establishment

Allow for all necessary preliminaries for the proper execution and completion of the works including, but not limited to:

· Mobilisation and demobilisation to and from site
· Provision of temporary electricity, potable water and lighting
· Provision of scaffolding and access equipment
· Area demarcation and temporary protection works
· Survey and verification of existing structure prior to commencement of works

2.2 AML Compliance Requirements

Allow for compliance with AML Co Ltd requirements in respect of:

· Health & Safety
· Security procedures
· Environmental protection measures
· Access permits
· Interfacing and coordination with relevant Authorities

3. NEW WORKS

3.1 Roof Sheeting

3.1.1 Metal Roof Covering

Supply and install galvanised mild steel roof sheeting, 0.75 mm thick, prepainted both sides or approved equivalent, profiled to Client’s approval, complete with all necessary accessories and fixings including:


· Approved self-tapping screws
· Washers, caps and malakoffs
· Waterproof adhesive strips to side and end laps
· Necessary cutting using nibbler cutter only
· Waste, protection and ancillary items

All works shall be carried out in accordance with manufacturer’s specifications and to the approval of the Client/Engineer.

Locations include:

· Roof covering with pitch
· Extra over for crimping of sheets

3.1.2 GMS Capping and Flashing

Supply and install prepainted galvanised mild steel capping/flashing, 0.75 mm thick and 600mm girth, complete with:

· Waterproof band tape
· Self-adhesive foam closure strips
· Standard closures to underside
· All necessary fixings and accessories

All works shall comply with manufacturer’s specifications and Client’s approval.

Locations include:

· Hip capping
· Hip flashing
· Barge capping

3.2 Structural Metal Works

3.2.1 Metal C-Purlins

Supply and fix hot dipped galvanised after manufacture mild steel C-purlins size 100 mm x 100 mm x 2.4 mm thick.

Rate shall include:

· Cutting to required sizes
· Rounding of sharp edges
· Continuous fillet welds where required
· Brush galvanising of site welds
· Fixing with appropriate bolts
· Application of:
· One coat galvanised iron cleaner
· One coat etch primer
· Two coats enamel paint

All works to drawings and Client’s approval.
3.2.2 Metal Plates

Manufacture, supply and fix mild steel plates size 100 mm x 100 mm x 5 mm thick, hot dipped galvanised after manufacture.

The works shall include:

· 6 mm continuous fillet welding
· Connection/anchor bolts M12
· Washers and nuts
· Cutting and preparation works
· Brush galvanising of welds

Rate shall also include application of:

· One coat galvanised iron cleaner
· One coat etch primer
· Two coats enamel paint

All works to drawings and Client’s approval.


LOT 2 – NEW METAL SHEETING AT POWER CENTRE

1. DISMANTLING WORKS

1.1 General

Carefully dismantle existing metal elements as described below and hand over reusable materials to the Client or cart away debris to an approved dumping site within 2 km from site unless otherwise specified.

The Contractor shall allow for:

· Temporary hoarding and protection to existing structures and surrounding installations.
· Safe removal and disposal of debris.
· No stacking of debris or dismantled materials outside allocated working areas.
· Leaving all surfaces clean and ready to receive new works.

1.2 Existing Metal Elements

The works shall include dismantling and removal of:

· Existing louvers
· Existing flashings
· Existing metal sheets
· Existing fixation fittings, screws and accessories



2. PRELIMINARIES & GENERAL

2.1 Site Establishment

Allow for all necessary preliminaries for the proper execution and completion of the works including, but not limited to:

· Mobilisation and demobilisation to and from site
· Provision of temporary electricity, potable water and lighting
· Provision of scaffolding and access equipment
· Area demarcation and temporary protection works
· Survey and verification of existing structure prior to commencement of works

2.2 AML Compliance Requirements

Allow for compliance with AML Co Ltd requirements in respect of:

· Health & Safety
· Security procedures
· Environmental protection measures
· Access permits
· Interfacing and coordination with relevant Authorities

3. NEW WORKS

3.1 Metal Sheeting Works

3.1.1 Metal Roof Covering

Supply and install galvanised mild steel roof sheeting, 0.75 mm thick, prepainted both sides or approved equivalent, profiled to Client’s approval, complete with all necessary accessories and fixings including:

· Approved self-tapping screws
· Washers, caps and malakoffs
· Waterproof adhesive strips to side and end laps
· Necessary cutting using nibbler cutter only
· Waste, protection and ancillary items

All works shall be carried out in accordance with manufacturer’s specifications and to the approval of the Client/Engineer.

Locations include:

· Roof covering with pitch to front of louvers
· Behind louvered vents – 1300 mm wide
· Included canopy – 600 mm wide



3.1.2 GMS Capping and Flashing

Supply and install prepainted galvanised mild steel capping/flashing, 0.75 mm thick and 600 mm girth, complete with:

· Waterproof band tape
· Self-adhesive foam closure strips
· Standard closures to underside
· All necessary fixings and accessories

All works shall comply with manufacturer’s specifications and Client’s approval.

Locations include:

· Cap flashing to metal sheet screen
· Flashing to U-shape purlins
· Gutter under metal louvers

3.2 Aluminium Gutters

Manufacture, supply and install coated colour aluminium gutters to Contractor’s design and in line with existing profile and appearance.

The works shall include:

· 3.5 mm thick aluminium sheeting
· Necessary stiffeners
· GMS brackets 25 mm x 5 mm thick
· All necessary accessories and fittings

All details shall be subject to Client’s approval.

Description:

· Aluminium gutter not exceeding 600 mm girth

4. REFIXING OF EXISTING METAL ELEMENTS

4.1 Existing Metal Elements

Carefully refix existing metal elements to their original positions.

The works shall include:

· Cleaning and sanding down surfaces
· Application of one coat galvanised iron cleaner
· One coat etch primer
· Two coats enamel gloss paint
· Replacement with new appropriate bolts and fixation fittings

Existing elements include:

· Existing metal louvers
· Existing barge flashing underneath front louvers

5. PROVISIONAL SUM

5.1 Treatment of Existing Metallic Structure

Chipping and removal of rust to existing metallic structures including application of:

· One coat galvanised iron cleaner
· One coat etch primer

All works to Engineer’s/Client’s approval.

5.2 Replacement of Rusted Fixings

Remove all rusted bolts, washers and nuts and replace with new galvanised steel bolts, washers and nuts of matching dimensions, all to Engineer’s/Client’s approval.

5.3 Anti-Bird Netting

Supply and install PVC mesh anti-bird netting to metal louvers including:

· GMS press plate 20 mm x 3 mm thick
· All necessary fixings and accessories

All works to Engineer’s/Client’s approval.


LOT 3 – NEW ROOF METAL SHEETING AT GROUND2AIR WORKSHOP

1. DISMANTLING WORKS

1.1 General

Carefully dismantle existing metal sheeting as described below and hand over reusable materials to the Client or cart away debris to an approved dumping site within 2 km from site unless otherwise specified.

The Contractor shall allow for:

· Temporary hoarding and protection to existing structures and surrounding installations.
· Safe removal and disposal of debris.
· No stacking of debris or dismantled materials outside allocated working areas.
· Leaving all surfaces clean and ready to receive new works.



1.2 Existing Metal Roofing Elements

The works shall include dismantling and removal of:

· Existing metal roof sheets
· Existing capping
· Existing flashing
· Existing fixation fittings, screws and accessories

2. PRELIMINARY & GENERAL

2.1 Site Establishment

Allow for all necessary preliminaries for the proper execution and completion of the works including, but not limited to:

· Mobilisation and demobilisation to and from site
· Provision of temporary electricity, potable water and lighting
· Provision of scaffolding and access equipment
· Area demarcation and temporary protection works
· Survey and verification of existing structure prior to commencement of works

2.2 AML Compliance Requirements

Allow for compliance with AML Co Ltd requirements in respect of:

· Health & Safety
· Security procedures
· Environmental protection measures
· Access permits
· Interfacing and coordination with relevant Authorities

2.3 Preliminary & General Items

The Contractor shall include in this Bill all costs deemed necessary for Preliminary & General (P&G) items required for the proper execution and completion of the project.

3. NEW WORKS

3.1 Roof Sheeting Works

3.1.1 Metal Roof Covering

Supply and install galvanised mild steel roof sheeting, 0.75 mm thick, prepainted both sides or approved equivalent, profiled to Client’s approval, complete with all necessary accessories and fixings including:

· Approved self-tapping screws
· Washers, caps and malakoffs
· Waterproof adhesive strips to side and end laps
· Necessary cutting using nibbler cutter only
· Waste, protection and ancillary items

All works shall be carried out in accordance with manufacturer’s specifications and to the approval of the Client/Engineer.

Locations include:

· Roof covering with pitch
· To RHS side wall
· To LHS side wall
· To end wall

3.1.2 GMS Capping and Flashing

Supply and install prepainted galvanised mild steel capping/flashing, 0.75 mm thick and 600mm girth, complete with:

· Waterproof band tape
· Self-adhesive foam closure strips
· Standard closures to underside
· All necessary fixings and accessories

All works shall comply with manufacturer’s specifications and Client’s approval.

Locations include:

· Barge capping to LHS side wall – girth not exceeding 700 mm
· Bottom flashing to LHS side wall – girth not exceeding 400 mm
· Gutter to front elevation – girth not exceeding 400 mm including 6 nr spouts for rainwater downpipes

3.2 Structural Metal Works

The following works shall be in hot dipped galvanised mild steel after manufacture.

Rates shall include:

· Cutting to required sizes
· Rounding of sharp edges
· Continuous fillet welds where required
· Brush galvanising of site welds
· Fixing with appropriate bolts
· Application of:
· One coat galvanised iron cleaner
· One coat etch primer
· Two coats enamel paint

All works shall be to drawings and Client’s approval.

3.2.1 Metal Z-Purlins

Supply and fix metal Z-purlins size 180 mm x 50 mm x 2.4 mm thick to RHS side wall.

3.2.2 Metal Z-Purlins

Supply and fix metal Z-purlins size 180 mm x 50 mm x 2.4 mm thick to LHS side wall.

3.2.3 Metal Z-Purlins

Supply and fix metal Z-purlins size 250 mm x 90 mm x 2.4 mm thick to LHS end wall.

3.2.4 Metal Z-Purlins

Supply and fix metal Z-purlins size 250 mm x 90 mm x 2.4 mm thick to roof.

3.2.5 Metal Z-Purlins

Supply and fix metal Z-purlins size 250 mm x 90 mm x 2.4 mm thick to front elevation.

4. PROVISIONAL SUM

4.1 Treatment of Existing Metallic Structure

Chipping and removal of rust to existing metallic structures including application of:

· One coat galvanised iron cleaner
· One coat etch primer

All works to Engineer’s/Client’s approval.

4.2 Replacement of Rusted Fixings

Remove all rusted bolts, washers and nuts and replace with new galvanised steel bolts, washers and nuts of matching dimensions, all to Engineer’s/Client’s approval.


SPECIFICATIONS & SAMPLE FOR MATERIALS 

The successful bidder should submit specifications and sample of materials to be used for approval prior to start of works.

AS BUILT DRAWINGS 

The Contractor shall submit As Built drawings within 28 days from the issue of taking over certificate.




B. STRUCTURAL STEEL WORK SPECIFICATIONS

1.0.0 Quality of Materials and Workmanship

1.1.0 The quality of all materials and workmanship used in the execution of this contract shall comply with the requirements of most recent issues of the following British Standards and Codes of Practice, including all amendments to date of calling for tenders:


	BS 4360
	Weldable Structural Steels

	BS 5950
	Structural Use of Steelwork in Building

	BS 4848 and            BS 4 (Part 1)
	Hot Rolled Structural Steel Sections

	BS 4848 (Part 2)
	Hollow Sections 

	BS 4848 (Part 4)
	Equal and Unequal Angles

	BS 5135
	Arc Welding of Carbon and Carbon Manganese Steels

	BS 639
	Covered Carbon and Carbon Manganese Steel Electrodes for the Manual Metal Arc Welding

	BS EN 288 (Part 3)
	Welding Procedure Tests for the Arc Welding of Steel 

	BS  2600 (Part 1)
	Radiographic Examination of Fusion Welded Butt Joints in Steel

	BS 4190
	ISO Metric Black Hexagon Bolts, Screws and Nuts

	BS 3692
	ISO Metric Precision Hexagon Bolts, Screws and Nuts

	BS 4320
	Metal Washers for General Engineering Purposes Metric Series

	BS 5493
	Code of Practice for Protective Coating of Iron and Steel Structures against Corrosion

	BS 729
	Hot Dip Galvanized Coatings on Iron & Steel Articles

	BS 2569 (Part 1)
	Sprayed Metal Coatings.  Protection of Iron and Steel by Aluminium and Zinc against Atmospheric Corrosion

	BS 5531
	Code of Practice for Safety in Erecting Structural Frames



The Contractor is required to submit a certificate of compliance from his supplier stating that the material to be supplied to him for the project shall meet the requirements of the relevant specifications mentioned above, similarly, certificate for the manufacture/ fabrication / galvanizing, etc. should be submitted; all before ordering.

Contractor is required to obtain test certificates for chemical analysis and mechanical test, including Chapter V notch impact test from steel maker for each batch of the steel supplied to his fabricator and to submit the same to the Engineer for his written approval.

The Engineer may at any time require any materials to be tested in accordance with the requirements of the Standards listed above.  The cost of all successful tests shall be borne by the Client, but the Contractor shall, when required, promptly supply to the laboratory for testing at his own expense test pieces as required by the Engineer. The costs of tests on materials failing to comply with this standard shall be borne by the Contractor.  If in the opinion of the Engineer, faulty material and/or workmanship have been used in the Works, the Contractor may be directed to dismantle and cut out the parts concerned and remove them for examination and testing.  The cost of dismantling, cutting out and making good to the approval of the Engineer shall be borne by the Contractor, in addition to the costs due to delays, etc., all in accordance with the Conditions of Contract.

The test certificates of chemical analysis will give all necessary information including percentage of alloying elements to assist the fabricator of the Contractor to decide on precautions to be taken during welding.

1.2.0	Materials, fabrication and erection in hot rolled sections of structural steel work shall comply with BS 5950: Part 2: l985 and additionally unless where specified otherwise in this specification, the information given under Article 10.0.0 of this specification for each particular project is supplied to the Contractor for him to comply with, and for use by the Steelwork Contractor’s design as required in Appendix A.3 of this British Standard.

2.0.0 Fixing to Concrete

2.1.0 Contractor is to check and ensure that provision for tolerances shown on the drawings for connection to concrete are adequate for erection.  Contractor may propose to use at his cost appropriate diameter tubes in expanded metal covered with nylon mesh or removable appropriate diameter tubes for casting of the holding down bolts before grouting with cement sand mortar as per Clause 2.6 of Section 2 of British Standard BS 5950: Part 2.  The tolerance gap up to 25 mm between the base plate and the concrete top will be in approved thick fluid epoxy mortar instead of Portland cement grout so that the space is completely filled.  Gap greater than 25 mm will be filled as per the above-mentioned Clause of the British Standard.  Holding down bolts should not be grouted until steelwork has been corrected for all defective work, lined, plumbed and levelled.  All holding down bolts will have an additional lock nut.

3.0.0 Fabrication

3.1.0	Cutting and Bending

All members, plates, brackets, etc., shall be neatly and accurately sheared, sawn, or profiled to the required shape as shown on the drawings.  It will be free from burrs and distortion.  Cutting of sheet material up to 15mm thickness shall be by guillotine shear and/or by heavy duty shears. 

Thicker plates shall be cut by cold saw or abrasive wheel.  Manual oxyacetylene flame cutting will not be permitted.  Laser cutting for the hollow sections will be preferred.  Ends of sections (CHS) are required to be prepared by saddling machine, Muller or similar before welding.
If members or plates are bent or set, the bends or sets shall be correctly made to the radii or angles specified without leaving marks.  The material may be heated to permit this.  Material that has been heated shall be annealed to approval.

3.2.0	Punching & Drilling

Holes for black and high precision bolts shall be drilled or punched 2 mm larger in diameter than the bolt used.  Holes for high tensile friction grip bolts shall be drilled or sub-punched and reamed to 3 mm larger in diameter than the specified bolts sizes.

All drilled holes shall be parallel sided and shall be drilled with the axis of the holes perpendicular to the surface.  Badly drilled holes shall either be reamed out if approved and/or larger bolts fitted or otherwise as directed by the Engineer.  All rough arises shall be ground off.   Holes for bolts in material thicker than 8mm must be drilled.  When holes are drilled in one operation through two or more thicknesses of material, the parts shall be separated after drilling and all burrs removed before assembly.  Holes for bolts shall not be formed by a gas cutting process.

3.3.0 Holes of not less than 12 mm dia must be drilled at places to be agreed with the firm galvanising the finished product to allow for access to molten zinc, venting of hot gasses and subsequent draining of zinc.

3.4.0	Shop Assembly

Such assembly of unit in the shop as is specified or necessary before transporting to the site will be inspected by the Engineer before and after galvanising.  The work will be laid out in the shop or yard so that all parts are accessible for inspection and testing of the work. 

The Contractor shall furnish all facilities for inspection and testing of the work and he must notify with reasonable notice the Engineer on each occasion when material is ready for inspection.

3.5.0	  Storage & Handling

Fabricated steelwork must be stored clear of the ground and be kept clean.  Handle and store to avoid damage to steelwork and its protective coating.

3.6.0	Welding

All welding shall be carried out in strict accordance with the specified British Standard with electrodes also to specified British Standard.

Unless where shown otherwise all welds shall be of size not less than 8mm.  Welding on site is not permitted unless where shown specified as site welding on the drawings.

Fusion faces shall be free from irregularities such as tears, fins, etc., which would interfere with the deposition of weld metal.


Fusion faces shall be smooth and uniform and shall be free from loose scale, slag, rust, grease, paint and/or other deleterious material.

All welds shall be of acceptable types, shall be of the finished sizes specified, and shall be carried out in such sequence that minimum distortion of the parts welded results.  No welds less than four times the nominal fillet size shall be deemed capable of carrying load.

Preparation of edges for welding shall be carried out by planning or machine flame cutting.

Parts to be welded shall be maintained in their correct relative positions during welding by jigs.

Multiple run welds shall be carried out with each run closely following the previous run but allowing sufficient time for the proper removal of slag.	

The Contractor shall ensure that each run is inspected and any unsatisfactory weld cut out and remade to approval.

Welds in material 25 mm or greater in thickness shall be made by the Argon arc or similar approved process, and special precautions shall be taken to prevent weld cracking.

Unless otherwise shown, the minimum size of fillet/butt weld shall be 8mm.

On completion, welds shall present a smooth and regular finish.  Weld metal shall be solid throughout with complete fusion between weld metal and parent metal and between successive runs throughout the joint.

Defects shall be cut out and made good to approval in sound weld metal.

For butt welds to ensure full throat thickness at ends run on and run off plates are used. Butt welds in CHS or RHS shall be with backing plates of the thickness shown or of the thickness of the thicker member.  Materials of the plates should be same as that of materials welded.

No additional welds or tack welds other than shown on the drawings will be permitted without the written approval of the Engineer.

Contractor is required to submit and to arrange for testing at the workshop all at his cost, the evidence of competence of welders in accordance with the specified British Standard for the type of works of the project.

Contractor will be deemed to have allowed in his rate for fabrication costs for welding for radiographic tests in accordance with the specified British Standard Weld defect criteria C generally in accordance with Tables 18 and 19 of BS 5135 will be applicable.  

3.7.0	Bolting

All bolts used shall be of such length that at least two full threads is exposed beyond the nut after the nut has been tightened on washer/washers between bolt head/nut and the structural member.  Where a nut or bolthead would bear on an inclined surface, a bevelled washer of the correct shape shall be interposed between the two surfaces.  Bevelled washers shall not be allowed to get out of position during fabrication and erection and for this purpose may be spot welded to the steel surface.  Such spot weld will be treated as welding on site.  Washers for oversize/shaped holes shall be of thickness shown or that of the connecting plates.  No bolts used shall be less than 12 mm diameter.

Bolts, nuts and washers used shall be spun galvanised to have minimum coating of 85 microns and they shall be tapped lightly oiled after galvanising.

Seal bolt holes by an approved method (this will be deemed to have been included in the rate of fixing) to prevent access of moisture in hollow sections.  Contractor will submit the method for Engineer’s approval.

3.8.0	Marking

All members of the structure to be site assembled shall be match marked in accordance with the shop details and marking plans submitted for approval.  Members should not be marked with hard stamping indentation.

3.9.0	Protective Treatment

After manufacturing the lengths of the sections between the bolted connections shown on the drawings are required to be hot dipped galvanised to BS 729 with minimum coating thickness of 85 microns. 

The steel is cleaned of foreign material, scale and roughen surface.  It may be necessary to use an approved blast cleaning to Engineer’s approval before acid pickling by immersing in a bath of suitably inhibited acids which dissolve or remove mill scale and rust to achieve galvanising to BS 729.

Double bath dipping can be used when the length or width as shown on the drawing exceeds the size of the bath.

Inside of hollow section shall be dry and clear of all debris before sealing holes left for ventilation, etc. as per section 4.6 of the British Standard.  Contractor is deemed to have included the cost of such works in the tendered price.

Where the protective surface is damaged by handling tack welding for temporary members, cutting, drilling, welding, etc., it shall be cleaned with an approved blasting before treating the surface with zinc metal spray coating to BS 2569: 
Part 1.  Such coating will be of 170 microns thickness.

All architectural/structural steel section, wire rope not shown as structural members on structural drawings, etc., shall have protected hot dipped galvanised coating and finished as structural members.  Steel windows forming part adjacent to the roof light or wall structure shall be hot dipped galvanised as structural members including its fixings.

Painting to structural members shown on drawings is not required unless specified after galvanising.  But cleaning of them without damaging protective treatment should be carried out at no costs.

4.0.0	Finishes

4.1.0	Paints

All paints are to be supplied to meet the requirements of the appropriate British or other specified Standard by a supplier approved in writing by the Engineer. 

Paints are to be delivered to the site or the Structural Contractor’s works in the original containers as supplied by the manufacturer with seals unbroken and are to be used in strict accordance with the manufacturer’s instructions.  Manufacturer’s representatives are to be free to visit the site and inspect materials and workmanship, and if necessary take samples of materials for laboratory analysis.

	Paints are not to be thinned unless instructed by the Engineer. 

	No external painting is to be carried out during rain or when rain is likely to occur before the paint has had time to dry.

	All surfaces are to be dry and free from moisture at the time of painting.

4.2.0	Preparation for Painting

	All structural steel shall be thoroughly scraped and wire brushed to remove mill scale and rust.  Dirt and grease or oil shall be washed off with white spirit and the steel allowed to dry.

4.3.0	Painting to Ungalvanised Surfaces

	A first coat of Red Lead type C Primer shall be applied in the works immediately the steel preparation has been completed, in accordance with the requirements specified in MS 13.  A minimum of 24 hours shall elapse before the steel is moved from its position whilst painting.

	After delivery to site, the steel shall be carefully examined and all areas where the priming coat has been damaged and/or where rust has developed shall be washed with white spirit and wire brushed as necessary and a further priming coat as for the first coat applied to completely cover the damaged areas.

	A minimum of 48 hours after any patching work has been completed, the whole of the steel shall be cleaned off with white spirit and 2nd coat of Red Lead Type C Primer of a different approved colour or shade from the first coat shall be applied and the painted steelwork left undisturbed for a further 48 hours.

	During erection, surface of steel which is to be in contact shall be painted with 1 further coat of primer as previously described and the surfaces brought together whilst the paint is still wet.
	
	After erection a third and finishing high gloss enamel (white) or other approved shade of colour to BS 4800 “Schedule of Paint Colours for Building Purposes”, meeting the requirements of SABS 630 “Decorative high gloss enamel paint for interior and exterior use” or a coat of Micaneous Iron Oxide is applied if noted on the drawing.
	Bolts, nuts and washers, etc, shall, after erection is completed to approval, be carefully degreased with white spirit and painted as for steelwork.

	Steel purlins and sheeting rails shall generally be pained as for steelwork except for purlins and rails supporting aluminium sheeting, when the following specification shall be used:

	1st Coat    - Red Oxide Zinc Chromate Primer
	2nd Coat   - Red Oxide Zinc Chromate Primer
	3rd Coat   - Approved Aluminium Paint	

	The interior of mild steel gutters shall be prepared as previously described and painted with 2 coats of Epilac Coal Tar Epoxy Paint.

4.3.1	Painting to Galvanised Surface

(a) Surfaces shall be thoroughly cleaned wire brushed to remove scales.  Dirt and grease or oil shall be washed with hot water.

(b) Apply 1 coat of etching primer (with min 15% phospheric acid) to enable sufficient adhesion of the subsequent paint.

(c) Apply 1 coat of calcium plumbate primer in accordance with “SABS 912”

(d) Apply 2 coats of white high gloss enamel in accordance with SABS 630 “Decorative High Gloss Enamel Paint for Interior and Exterior Use” of an approved shade of colour to BS 4800.

	Allow 24 hours intervals between each coat.



Airport Constraints

As the works shall be carried out in a controlled zone, the successful bidder will be required to ensure the followings: 

· The site shall remain accessible to any access and egress for airport vehicles at all times.  

· All works to be carried out within approved time slot agreed by AML.

· All portion of works to be secured with appropriate hoardings, warning signs, barricades and the like.

· To adhere with reasonable temporary suspension of works as directed by relevant authorities.


General Procedures

· The Successful Bidder shall submit a Commissioning Certificate after successful completion.

· All Contractors’ personnel shall follow a security and safety briefing session prior to commencement of works on site. Contractor shall abide to all airport standing procedures.

· All personnel on site should wear PPE pertaining to the works as applicable.

· All materials to be used for completion of these works shall be provided by the Contractor. 

· The site must be kept clean during and after works are carried out. and necessary precautions to be taken to avoid falling of paints on existing building structure.

· All debris and left overs shall be disposed daily or regularly according to Rules and Regulations pertaining to the prevailing Laws on Environment, and AML shall not be held responsible in any circumstances in case the Contractor contravenes such Rules & Regulations.

· Contractor must note that all quantities in the BOQ are indicative and payment will be based on measurement after completion of works.

· The Contractor will be required to submit a programme of works for approval by AML prior to start of works.

· All completed works will be checked and commissioned by the Employer’s representatives and any necessary corrective works to meet specified requirements, must be carried out by the Contractor without any additional cost.

· In case of force majeure, Contractor will be informed by AML so as not to mobilise for works.

· The Successful bidder shall have to submit Clean Certificates of Character of its personnel involved in this contract prior to mobilization on site. Non-submission of same shall lead to termination of Contract.

List of Annexes

· Annex 1 – Drawings 
· Annex 2 – Photographic illustrations of sites Lot 1, 2 & 3
· Annex 3 - General Conditions of Contract


List of Appendices

· Health & Safety Requirements for Construction Contractors
· Security Procedures for Works within the Security Restricted Area
· Procedures for Application of Access Permit for the Security Restricted Area
· Cyclone Procedure



Section IV: General Conditions of Contract and Particular Conditions of Contract
Any resulting Contract shall be placed by means of a Letter of Acceptance and shall be subject to the General Conditions of Contract (GCC), for the Procurement of Works except where modified by the Particular Conditions of Contract below. 
Procurement Reference Number: ONB/WK/TSD/VB/CL/25/008 RL1 (14 Oct) TC

The clause numbers given in the first column correspond to the relevant clause number of the General Conditions of Contract.
Particular Conditions of Contract

	A. General

	GCC 1.1 (r)
	The Employer is Airports of Mauritius Co Ltd (AML).

	GCC 1.1 (v)
	The Intended Completion Date for the whole of the works shall be 90 calendar days as from the start date.

	GCC 1.1 (y)
	The Project Manager contact details shall be communicated after award of the Contract.

	GCC 1.1 (aa)
	The sites are located at (i) Power Centre, (ii) Mechanical Shed opposite AML Store and (iii) Aircraft Discharge Shed at SSR International Airport, Plaine Magnien.


	GCC 1.1 (dd)
	The Start Date shall be the date specified in the Notice to Commence.

	GCC 1.1 (hh)
	The work consists of Metal Roof Refurbishment works at Power Centre and Sheds at SSRIA.

	GCC 2.2
	N/A

	GCC 2.3(i)
	The following documents also form part of the Contract:

(a) Contract Agreement
(b) Letter of Acceptance
(c) Contractor’s Bid
(d) Particular Conditions of Contract
(e) General Conditions of Contract
(f) Specifications
(g) Drawings
(h) Bill of Quantities

All other correspondence related to this bidding exercise.


	GCC 3.1
	The language of the Contract shall be in English
The law that applies to this Contract is the law of Mauritius.



	GCC 5.1
	The Project Manager may delegate any of his duties and responsibilities to Representative of AML. 

	GCC 8.1
	N/A

	GCC 13.1
	Except for the cover mentioned in (a) and (d)(i) hereunder, the other insurance covers shall be in the joint names of the Contractor and the Employer and the minimum insurance amounts shall be as follows:

(a) for the Works, Plant and Materials: MUR 6 Million

(b) for loss or damage to Equipment: MUR 5 million

(c) for loss or damage to property (except the Works, Plant, Materials, and Equipment) in connection with Contract: MUR 5 million

(d) for personal injury or death: MUR 5 million (per person and per occurrence): 

(i) of the Contractor’s employees
(ii) of other people

The Contractor shall choose to take the insurance covers indicated above as separate covers or a combination of the Contractor’s All Risks coupled with AML’s liability and First Loss Burglary, after approval of AML.

All insurance covers shall be of nil or the minimum possible deductibles at sole expense of the Contractor.

The insurance policies shall be extended to cover for any extension of the intended completion date or due to delay by the contractor up to the end of the defects liability period of the works.

	GCC 14.1
	Please refer to drawings and appendices for site data.

	GCC 20.1
	The Site Possession Date(s) shall be communicated in the kick-off meeting.

	GCC 23.1 &
GCC 23.2
	No Adjudicator shall be appointed for this Contract.

	GCC 24.
	In case a dispute of any kind arises between the Employer and the Contractor in connection with, or arising out of, the contract or the execution of works or after completion of works and whether before or after repudiation or other termination of Contract, including any dispute as to any opinion, instruction, determination, certificate or valuation of the Employer’s Representative, the matter in dispute shall, in the first place, be referred in writing to the employer’s representative, with a copy to the other party.

The Employer and the Contractor shall make every effort to resolve the dispute amicably by direct informal negotiation. If, after twenty-eight (28) calendar days, the parties have failed to resolve their dispute or difference by such mutual consultation, then either the Airports of Mauritius Co Ltd or the Contractor may give notice to the other party of its intention to refer the matter to:- “commence arbitration, as hereinafter provided, as to the matter in dispute, and no arbitration in respect of this matter may be commenced unless such notice is given to the other party of its intention to refer the matter to “the competent courts of Mauritius”.

	B. Time Control

	GCC 25.1
	The Contractor shall submit for approval a Program for the Works within 7 calendar days from the date of issue of the Letter of Acceptance.

	GCC 25.3
	The Contractor shall submit to the Project Manager for approval an updated Program within 14 calendar days from the date of issue of the Letter of Acceptance.

	C. Quality Control

	GCC 33.1
	The Defects Liability Period (DLP) shall be 365 calendar days as from the site handing over date. The amount withheld shall be 10% of the contract value or Retention Money from each payment. 5% will be released on completion of project and remaining 5 % at end of DLP.

	GCC 34.1
	Should any defect arise during the Contractual period or up to the end of the Defects Liability Period and subsequently, the Contractor fails to correct the Defect within the time specified in the Project Manager’s notice, this shall constitute a breach of the Contractor’s obligations under this Contract.
The Project Manager shall assess the cost of having the defect corrected and recover the money from outstanding payment or from the Performance Security.

	GCC 39.7
	Interim Payment for Plant and Material on site is not applicable for this Contract.

	D. Cost Control

	GCC 40.1
	N/A

	GCC 41.1 (l)
	Exceptionally adverse climatic conditions, defined as any one of the following events:
(i) minimum of 100 mm rainfall or 2 hours continuous heavy rainfall recorded in one day at the nearest approved Rain Station,
(ii) Torrential rain declared by the Meteorological Department of Mauritius,
(iii) Cyclone warning Class III or Class IV.

	GCC 43.1
	The currency shall be Mauritian Rupees (MUR).

	GCC 44.1
	The Contract is not subject to price adjustment.

	GCC 45.1 & 45.2
	10 %, of the payment being effected shall be retained and 5% of the retention money shall be released following the Certificate of completion.  

	GCC 46.1
	The Liquidated Damages for the whole contract shall be 2% per week or part thereof and same would be applied per work order.

The maximum amount of Liquidated Damages for the whole of the Works shall be 10% of the Contract Value.

	GCC 47.1
	N/A

	GCC 48.1
	The Advance Payment shall be 10% of Contract Value excluding any Provisional & Contingencies sums, upon submission of a Bank Guarantee as per Advance Payment Security form hereunder.

	GCC 48.3
	N/A

	GCC 49.1
	The Performance Security amount shall be 10% of the Contract Value excluding any Provisional & Contingencies sums and VAT, and shall be submitted as per Performance Security form hereunder.


	E. Finishing the Contract

	GCC 56.1
	The date by which “as built” drawings are required, shall be 28 calendar days after completion of work.

	GCC 57.2 (g)
	The maximum number of days is: 30 calendar days.

	GCC 59.1
	The percentage to apply to the value of the work not completed, representing AML’s additional cost for completing the Works is 10%.



Section V- Contract forms

Performance Security

...............................Bank/Insurance Company’s Name and Address of Issuing Branch or Office….....................................................

Beneficiary: .............................................Name and Address of Employer................................................................
Date..............
PERFORMANCE GUARANTEE No.: ..........................................................................................
We have been informed that ..................................[name of the Contractor]	(hereinafter
called "the Contractor") has entered into Contract No.............[reference number of the Contract] ............
dated.	with you, for the execution of	[name of Contract and brief description of Works]
.	(hereinafter called "the Contract").


Furthermore, we understand that, according to the conditions of the Contract, a performance security is required.


At the request of the Contractor, we ................................. [name of Bank/Insurance Company]	hereby
irrevocably undertake to pay you any sum or sums not exceeding in total an amount of	[amount
in figures (amount in words)]	such sum being payable in the types and proportions of
currencies in which the Contract Price is payable, upon receipt by us of your first demand in writing accompanied by a written statement stating that the Contractor is in breach of its obligation(s) under the Contract, without your needing to prove or to show grounds for your demand or the sum specified therein.


This guarantee shall expire and returned to us not later than twenty-eight calendar days from the date of issuance of the Defects Liability Certificate, calculated based on a copy of such Certificate which shall be provided to us, or on the................................day of ..................................,	,
whichever occurs first. Consequently, any demand for payment under this guarantee must be received by us at this office on or before that date.



…	Seal of bank/Insurance Guarantee and



Signature(s).............................................................

Advance Payment Security
[Bank’s/ Insurance Company’s Name, and Address of Issuing Branch or Office]

Beneficiary: .................................. [Name and Address of Employer] ..................................... Date: ............................................................................................................................................ Advance Payment Guarantee No.: ..........................................................................................
We have been informed that . . .. . [name of the Contractor] . . . . .	(hereinafter called “the Contractor”) has entered into Contract No. . . . . . [reference number of the Contract]	dated
. . . . . .. . with you, for the execution of	[name of Contract and brief description of Works] .
.	(hereinafter called “the Contract”).
Furthermore, we understand that, according to the Conditions of the Contract, an advance payment in the sum . . . . . [name of the currency and amount in figures] 1. . . . . . (.	[amount in words] .
.   ) is to be made against an advance payment guarantee.
At the request of the Contractor, we . . .. . [name of the Bank/Insurance Company]	hereby
irrevocably undertake to pay you any sum or sums not exceeding in total an amount of    [name
of the currency and amount in figures] *. . . . . . (. . . . . [amount in words]	) upon receipt by
us of your first demand in writing accompanied by a written statement stating that the Contractor is in breach of its obligation under the Contract because the Contractor used the advance payment for purposes other than the costs of mobilization in respect of the Works.
It is a condition for any claim and payment under this guarantee to be made that the advance payment referred to above must have been received by the Contractor on its account number . . .. . [Contractor’s account number] . . . . . at   [name and address of the Bank/Insurance Company]
. . . . . .
The maximum amount of this guarantee shall be progressively reduced by the amount of the advance payment repaid by the Contractor as indicated in copies of interim statements or payment certificates which shall be presented to us. This guarantee shall expire, at the latest, upon our receipt of a copy of the interim payment certificate indicating that eighty (80) percent of the Contract Price has been certified for payment, or on the . . . day of . . . . . .. , . . . . . 2, whichever is earlier. Consequently, any demand for payment under this guarantee must be received by us at this office on or before that date.
. . . . . . . . . . . . . . [Seal of Bank/Insurance Company and Signature(s)] . . . . . . . . . . . . . .

Note –
All italicized text is for guidance on how to prepare this demand guarantee and shall be deleted from the final document.
1 The Guarantor shall insert an amount representing the amount of the advance payment denominated either in the currency(ies) of the advance payment as specified in the Contract, or in a freely convertible currency acceptable to the Employer.
2 Insert the expected expiration date of the Time for Completion. The Employer should note that in the event of an extension of the time for completion of the Contract, the Employer would need to request an extension of this guarantee from the Guarantor. Such request must be in writing and must be made prior to the expiration date established in the guarantee. In preparing this guarantee, the Employer might consider adding the following text to the form, at the end of the penultimate paragraph: “The Guarantor agrees to a one-time extension of this guarantee for a period not to exceed [six months][one year], in response to the Employer’s written request for such extension, such request to be presented to the Guarantor before the expiry of the guarantee.
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